|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| http://clarktruck-in.com/wp-content/themes/vision/images/clarklogo.png | CLARK TRUCK EQUIPMENT105W. 580 N.CRAWFORDSVILLE, IN. 47933

|  |  |
| --- | --- |
| Phone: | (800) 382-0873 |
| Fax: | 765-362-4103 |

 | **Quotation****#02012023BJB****RE: TANDEM AXLE DUMP** |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NICK BROWNMcCORDSVILLE PUBLIC WORKS6280 W 800 NMcCORDSVILLE, IN 46055 |

|  |  |
| --- | --- |
| Phone:  | (317) 335-3493 |
| Fax:  | (317)414-0526 |
| Email: | nbrown@mccordsville.org |
|  |  |

 |

|  |
| --- |
| Date: 2/1/2023 |
| Rep.:  |
|  |
|  |

 |

**1 – HENDERSON MARK-E 14’ BODY PKG**; 52” SIDES CONSTRUCTED OF 10 GA 201 STAINLESS STEEL W/ SINGLE WELD ON HORIZONTAL REINFORCEMENT (10 GA 201SS); 3/16” AR400 FLOOR; 8” I-BEAM LONG SILLS; 52” AIR OPERATED ASPHALT TAILGATE WITH DOUBLE HORIZONTAL BRACES (10 GA 304SS) AND LIFT LOOP; M130-5.5-3 TRUNION MOUNTED DOUBLE ACTING FRONT MOUNT HOIST W/ INTERNAL DOGHOUSE (12”); ½ CAB SHIELD; TWO SAFETY PROPS; FOLDING LADDER ON DRIVER SIDE; ¼” REAR CORNER POSTS (201SS) w/ RECESSED LED S/T/T, AND LED AMBER STROBES; TWO PAIR MUD FLAPS; BACK UP ALARM; **34” TRUCK SIDE HUSTING HITCH W/ DOUBLE ACTING CYLINDER; CAB MOUNTED LIGHT BAR W/ PLOW LIGHTS AND BEACON STROBE; REAR TOW HOOKS; SURFACE MOUNTED STROBES MOUNTED IN FRONT GRILL AND REAR CORNER POSTS; ADJUSTABLE PINTLE HITCH ON ¾” PLATE W/ D-RINGS; 8” SPREADER APRON**

**FORCE AMERICA** CRANK MOUNTED PTO W/ DIRECT MOUNTED GEAR PUMP; 5100EX IN CAB CONTROLLER; 30 GAL. RESERVOIR w/ CABLE DRIVEN SHUT OFF VALVE, SIGHT GAUGE, RETURN LINE FILTER; THREE SECTION CONTROL VALVE TO OPERATE D/A HOIST, S/A PLOW RAISE, D/ PLOW ANGLE, PRE WET, AUGER AND SPINNER;

**PRICE INSTALLED: $62,923.00**

 **- HENDERSON 1' x 42" REVERSIBLE SNOW PLOW**; INTEGRAL SHIELD; FULL MOLDBOARD TRIP; LEVEL LIFT DESIGN; 0 GA GR50 ROLLED MOLDBOARD; 8 - /2" x 3 /2" VERTICAL RIBS; CONTINUOUS WELDED ONE PC MOLDBOARD; REINFORCED 4" 4" x 3/4" BOTTOM ANGLE; TOP ANGLE = 3 /2"x2 /2" x 3/8" W/ HOLES FOR MOISTURE ESCAPE; 2 HORIZONTAL BRACES; 5/8" x 8" ONE PC CUTTING EDGE; ORANGE IN COLOR; SEMI-CIRCLE IS A 4" x 4" x /2" ANGLE WELDED TO A 4" x 4" x 3/8" STRUCTURAL TUBING; PUSH FRAME WIDTH IS 96" - two 3" x 1 1/2" x 0" DOUBLE ACTING/REVERSING CYLINDERS (nitrided) CUSHION VALVE; **34" HUSTING HITCH (plow portion); 36” BLADE MARKERS**

**PRICE INSTALLED: $15,974.00**

**1 - HENDERSON 13’ FSH 62” SALT SPREADER;** 13’ SPREADER BODY; 10.7 CY CAPACITY; DUAL 7” AUGER DRIVEN; 10 GA 201 STAINLESS STEEL SIDES/ENDS, 7 GA 201 STAINLESS STEEL SILLS/FLOOR; 3.6:1 RATIO PLANETARY GEARCASE, SPINNER AND CHUTE; STANDARD TOP GRATES; INVERTED VEE IN 201 STAINLESS MATERIAL; HYDRAULIC LINES RAN TO THE BACK W/ QUICK DISCONNECTS;

**PRICE INSTALLED: $32,225.00**

 **TOTAL PACKAGE INSTALLED: $111,122.00**

ADDITIONAL OPTION (IF APPLICABLE)

* HENKE PLOW ILO HENDERSON **PRICE ADD: $650.00**

|  |  |
| --- | --- |
| Submitted by: **Jason Bridwell**Prices are F.O.B. Crawfordsville, In.Prices are good for 30 days.Any applicable taxes are additional.Approx. delivery is 30-36 weeks after receipt of order.Paint matches are approximate.A 3% fee will be added to all credit card charges. | Accepted By: |
| Thank you for your business. |