cid:image002.png@01D7B481.44FD22A0 **December 6, 2022**

**2024/25 Tandem Axle Dump, Snow & Ice Unit**

**Budgetary Proposal**

**14’-0” Stainless Steel Dump Body with 48” Sides, 54” Tailgate, 24” Cab Shield, 8”Spreader Apron, LED Light Kit. Inverted Trunnion Mounted Hoist and Body Prop.**

**Force America Central Hydraulic System – PTO-Pump Combo, VT35 Valve & Tank Enclosure with Add-A-Stack Bank, Single Axis Lever/Cable Control for Single Acting Hoist, Dual Axis Lever/Cable Control for Single Acting Plow Lift and Double Acting Plow Angle, EX5100 Electronic Spreader Controls. (35) Gallon Hydraulic Reservoir, 1-1/4” NPT Spin-on 10 Micron Filter Assembly with Visual Gauge. Hoses, Fittings, Quick Disconnects, and Hydraulic Fluid.**

**Henke 11 Foot x 42” Reversible Snowplow with Integral Shield Moldboard, 34” Husting Hitch with Thrust Arm Mount Brackets. Single Acting Lift and Double Acting Angling Cylinders. Rubber OEM Deflector and Plow Markers.**

**Hi-Way Model E2020 A2 - 13 Foot Stainless Steel, 10.1 Cubic Yard, Hydraulic Salt Spreader, with Dual Auger Feed.**

**3/4” Hitch Plate with D-Rings, 7 Way RV Trailer Plug, Mud Flaps, and all Miscellaneous Installation Materials.**

**Warning Light Package – Strobe Lights in Rear Corner Posts of Dump Body, Grill Mounted Strobes, Cab Mounted Light Bar with Beacon Strobes and LED Plow Lights.**

**We are pleased to project the above equipment installed in early 2025 for:**

**$ 162,000.00**

**Submitted To:**

**Nick Brown, Town of McCordsville – Public Works Department**

**Submitted By:**

**Tim Brattain, Territory Sales Manager Reading Truck - Indianapolis**

**317-914-3893 tbrattain@readingtruck.com**